[image: BBM_LOGO]
[image: BBM_LOGO]BBM-BIM | BBM-STD-93-CODE_DICTIONARY-V0.2


Code dictionary
Linked copies: ID STD-93 · TBP page · BABOOM edition · ArchHub: BABOOM companion
BBM-STD-93-CODE_DICTIONARY-V0.2 | Office standard | 5 November 2026 | V0.2 | Private controlled WIP draft for office review
	Version
	Date
	Change

	V0.1
	2026-11-04
	First issue: closes audit res-026 rows G007, G021, G026, G083, G200, G209, §1.3 "Single code dictionary" and the §1.4 contradictions on discipline/​role codes, suitability codes, gate outcome, review tiers, gate list and approval status vocabulary (O-DEC-103, 104, 107, 108, 109, 110, 113) + cross-doc pointer pass (gate map to the eight Manual §2.1 gates and BBM-STD-12 C5 short form, trade-alias map incl. DU/​WU -> C/​CIV per O-DEC-128, ISO 13567 agent code, Superseded aligned with BBM-STD-12 C4) + template alignment (O-DEC-142..148) + folder names without dots (O-DEC-149)

	V0.2
	2026-11-05
	§2.2 container-name token lists CLIENT, ORG, PROJ, VOLUME, LEVEL, TYPE with patterns, office rules and validity (O-DEC-162); §2.3 QMS checklist workbook codes (O-DEC-163)



1 Purpose and authority
This is the ONE office code dictionary. It replaces the code lists in BBM-STD-51 §4 (ROLE and suitability rows), BBM-STD-66 §1 (discipline designators), and Manual V0.5 §12.1 (folder discipline codes) and §12.3 (view and sheet discipline tokens); BBM-STD-50 and BBM-STD-68 use these codes (O-DEC-103). Those documents keep a pointer to this dictionary and, where needed, the local subset they use; they define no code of their own. The BIM Manager maintains this dictionary; a new code or meaning needs a ChangeID in BBM-STD-51 and a revision here.
Codes in this document are office codes. When a client or authority imposes another code set, the project records a one-to-one mapping in the BEP using the mapping columns below; issued literals are never renamed.
2 Discipline and role codes (O-DEC-103)
	Discipline
	3-letter code (views, folders, clash sets, QA, issue tracker)
	1-letter ROLE (file names, sheet prefix)
	Folder code
	Sheet prefix
	Issue-tracker value
	When a client imposes the UK National Annex role codes

	Architecture
	ARC
	A
	00-ARC
	A
	ARC
	A

	Structure
	STR
	S
	01-STR
	S
	STR
	S

	Mechanical
	MEC
	M
	02-MEC
	M
	MEC
	M

	Electrical
	ELE
	E
	03-ELE
	E
	ELE
	E

	Landscape
	LSC
	L
	04-LSC
	L
	LSC
	L

	Plumbing /​ public health
	PLU
	P
	05-PLU
	P
	PLU
	P

	Fire & Life Safety
	FLS
	F
	06-FLS
	F
	FLS
	Y (specialist designer): in the UK National Annex "F" means facilities manager, so FLS is not sent as F

	Interiors
	INT
	I
	07-INT
	I
	INT
	I

	Civil
	CIV
	C
	08-CIV
	C
	CIV
	C

	Survey
	SUR
	G
	09-SUR
	G
	SUR
	G

	Cost /​ quantities
	QTY
	Q
	10-QTY
	Q
	QTY
	Q

	Contractor
	CON
	W
	11-CON
	W
	CON
	W

	General /​ multi-discipline
	GEN
	Z
	12-GEN
	Z
	GEN
	Z



Rules:
•  Published library family names keep their own tokens (BBM-STD-69 §2): the G in title blocks BBM-G-TTB-A0…A3 is the library's general token, not the Survey ROLE G (O-DEC-144).
•  LSC = Landscape and FLS = Fire & Life Safety everywhere. "LSC: Life Safety and Code" is wrong and is not used.
•  Extra disciplines are added per project at the next free code (next free 3-letter code, 1-letter ROLE not yet used in the table, next folder number), recorded here before first use.
•  The UK National Annex column is a mapping for appointments that impose it; letters other than FLS are sent unchanged, checked against the client's annex code list at appointment.
•  Legacy aliases map one-to-one and are not used for new work: MECH → MEC; ELEC (view root and folder 03-ELEC) → ELE / 03-ELE; LND → LSC; ID → INT; "MEP" is an umbrella label for MEC + ELE + PLU, not a code; a legacy MEP view root maps to MEC, ELE or PLU per view content.
•  Folder numbers 00–04 keep the existing project folder order; 05–12 are allocated by this dictionary (O-DEC-137). The table lists disciplines in folder-number order.
•  Folder codes are written NN-CODE with a hyphen, never a dot (O-DEC-149). They sit, with the same numbers in the same order, under every data type in every state of the one project folder tree in Manual V0.5 §12.1.
•  File names: the 8-token external identity CLIENT-ORG-PROJ-VOLUME-LEVEL-TYPE-ROLE-NUMBER.ext uses the 1-letter ROLE (O-DEC-102). View names DISC-LEVEL[-ZONE]-TYPE-DESC use the 3-letter code (e.g. ARC-L02-PLAN-LAYOUTS, MEC-Z03-3D-COORD). Sheet numbers DISC-CAT-INDEX use the sheet prefix.
•  ISO 13567 agent responsible (2 characters, BBM-STD-66 §1.1 export mapping): the 1-letter ROLE followed by a hyphen (e.g. "A-", "F-"), unless the recipient's mapping table defines other values (O-DEC-141).
2.1 Clash trade aliases
The BBM-STD-50 office trade codes are selection aliases, not ROLE codes. Each maps to exactly one code here; the selection scope of each trade stays in BBM-STD-50 §4.
	Trade alias
	Meaning
	ROLE
	3-letter code

	AR
	Architecture
	A
	ARC

	ID
	Interiors
	I
	INT

	ST
	Structure
	S
	STR

	ME
	Mechanical
	M
	MEC

	EL
	Electrical
	E
	ELE

	LI
	Lighting
	E
	ELE

	WS
	Water services
	P
	PLU

	DR
	Drainage
	P
	PLU

	FF
	Fire protection
	F
	FLS

	LS
	Landscape
	L
	LSC

	CI
	Civil
	C
	CIV

	DU
	Dry utilities (external networks)
	C
	CIV

	WU
	Wet utilities (external networks)
	C
	CIV



DU and WU are external utility networks and take the civil role C / CIV (O-DEC-128). Where a building-services team produces a utility network, the project annex records the override against this table. A new trade alias needs a row here before it is used in a clash set.
2.2 Container name tokens (O-DEC-162)
The external container name CLIENT-ORG-PROJ-VOLUME-LEVEL-TYPE-ROLE-NUMBER.ext (Manual V0.6 §12.3, O-DEC-002, O-DEC-102) takes its token values from these lists. The information manager records every allocated value in the project naming register at mobilisation. Each token is valid from mobilisation (the first container, Stage 0/1); a value is never changed or reused after first issue (the O-DEC-124 principle). A client- or authority-imposed list replaces a token list for that project through a one-to-one mapping in the BEP. Examples are synthetic.
	Token
	Pattern
	Office rule
	Example

	CLIENT
	^[A-Z0-9]{2,6}$
	The client's own code where the appointment gives one; otherwise three letters allocated at mobilisation from the client's registered name, unique in the office project register
	CLI

	ORG
	^[A-Z0-9]{2,6}$
	Originator of the container. This office is BABOOM (the office prefix of every BBM-STD document and of the published library series, O-DEC-144); every other appointed party gets one code in the project naming register
	BABOOM

	PROJ
	^[A-Z0-9]{2,6}$
	The client's project code where given; otherwise the office job number P001–P999 from the office project register, never reused
	P001

	VOLUME
	ZZ, XX or [0-9]{2}
	ZZ = all volumes /​ whole project; XX = no volume applies; 01–99 = a building, block, zone or system listed with its name in the project volume register
	01

	LEVEL
	ZZ, XX, GF, RF, [0-9]{2}, B[0-9]{1,2} or M[0-9]{1,2}
	ZZ = multiple levels; XX = no level applies; GF = ground; 01–99 = floors above ground; B1, B2 … = basements; M1, M2 … = mezzanines; RF = roof. Each value is listed with its Revit level name and elevation in the project level register. The view LEVEL token (L01, LRF, ALL) is a separate grammar
	03

	TYPE
	^[A-Z0-9]{2}$, from the list below
	Information type of the container. A new type needs a row here before use
	M3

	ROLE
	^[ASMEPFLICGQWZ]$
	§2
	A

	NUMBER
	^[0-9]{4}$
	Sequence per CLIENT-ORG-PROJ-VOLUME-LEVEL-TYPE-ROLE, from 0001, never reused
	0001



Validator regexes: VOLUME ^(ZZ|XX|[0-9]{2})$; LEVEL ^(ZZ|XX|GF|RF|[0-9]{2}|B[0-9]{1,2}|M[0-9]{1,2})$; CLIENT, ORG and PROJ ^[A-Z0-9]{2,6}$. The Manual §12.3 container regex checks lengths; these lists check values.
Information types (UK National Annex information-type list via the IMI Framework, adopted as office list):
	Code
	Information type
	Code
	Information type

	AF
	Animation
	MI
	Minutes /​ action notes

	BQ
	Bill of quantities
	MR
	Model rendition

	CA
	Calculations
	MS
	Method statement

	CM
	Combined (federated) model
	PP
	Presentation

	CO
	Correspondence
	PR
	Programme

	CP
	Cost plan
	RD
	Room data sheet

	CR
	Clash rendition
	RI
	Request for information

	DB
	Database
	RP
	Report

	DR
	2D drawing
	SA
	Schedule of accommodation

	FN
	File note
	SH
	Schedule

	HS
	Health and safety
	SN
	Snagging list

	IE
	Information exchange file (e.g. COBie)
	SP
	Specification

	M2
	2D model
	SU
	Survey

	M3
	3D model
	VS
	Visualisation



Example container name (synthetic): CLI-BBM-P001-01-03-M3-A-0001.ifc.
2.3 QMS checklist workbook codes (O-DEC-163)
Checklist IDs read <workbook>-<sheet>-<nn> (O-DEC-151). The workbook codes and their folders in BABOOM-BIM-STANDARD\07-QA-QC:
	Code
	Workbook
	Folder
	Procedure owner

	DR
	Design review
	02-DESIGN-REVIEW
	BBM-STD-97 QP-03 /​ QP-04

	PR
	Proposals
	03-PROPOSALS
	BBM-STD-97

	SP
	Specifications
	04-SPECIFICATIONS
	BBM-STD-97

	SU
	Sustainability
	05-SUSTAINABILITY
	BBM-STD-97

	SB
	Authority submissions
	06-SUBMISSIONS
	BBM-STD-97

	SV
	Site supervision
	07-SUPERVISION
	BBM-STD-97

	DC
	Document control
	08-DOCUMENT-CONTROL
	BBM-STD-97

	QA
	QMS audit
	09-AUDIT
	BBM-STD-96



The BIM checklist in 01-BIM (BBM-STD-68) keeps its sheet prefixes MH, IC, DS, DI, AR, ID, LS, ST, ME, AU and IS. SU here is a workbook code, never a suitability code (SU-…, §3).
3 Suitability codes (O-DEC-104)
Office suitability codes are SU-WIP, SU-COORD, SU-INFO, SU-REVIEW and SU-ISSUE only. "S1"-style codes are not office suitability codes (in this office "S1" is issue severity, §8).
	Office code
	Meaning
	CDE state where used
	Maps to UK National Annex code when a client imposes it

	SU-WIP
	Team work in progress
	WIP
	S0

	SU-COORD
	Shared for coordination
	Shared
	S1

	SU-INFO
	Shared for information /​ reference
	Shared
	S2

	SU-REVIEW
	Shared for review and comment, or submitted for stage, PIM or AIM authorisation
	Shared
	S3; S4 when the client's annex calls the purpose stage approval; S6 /​ S7 when submitted for PIM /​ AIM authorisation

	SU-ISSUE
	Authorised for the defined use (tender, construction, record)
	Published
	A1…An (authorised and accepted) or B1…Bn (partially authorised, with comments) per the recipient's decision; CR for an as-constructed record



The meaning of each UK National Annex code is taken from the edition named in the client's appointment, checked at appointment and recorded in the BEP. SU-ISSUE does not prove statutory approval or recipient acceptance.
Revision forms (O-DEC-113): office revisions are per container, R00 initial WIP, then R01, R02 onward; never recycled; an unchanged container keeps its revision; no pack-wide monotonic revision. When a client imposes the UK National Annex forms, the project alias table maps each office revision to the client form (preliminary P-series for Shared, contractual C-series for Published, with any sub-version form the client specifies); the mapping is recorded once and never recalculated.
4 CDE states
	State
	Meaning

	WIP
	Work in progress inside the task team

	Shared
	Checked and shared with other task teams or the appointing party for the stated suitability

	Published
	Authorised for use; formal delivery is the transition to Published after authorisation (O-DEC-117)

	Archive
	Retained record of superseded or completed information (one spelling: Archive, folder 04-ARCHIVE)



Each state has one state folder in the project folder tree: 01-WIP, 02-SHARED, 03-PUBLISHED, 04-ARCHIVE (Manual V0.5 §12.1, O-DEC-149). A folder location alone does not prove the state, and the state is distinct from the suitability code.
5 Gate outcomes (O-DEC-107)
	Letter
	Meaning

	A
	Accepted for the stated purpose without required changes

	B
	Accepted for the stated purpose with listed non-blocking comments, owners and dates; B cannot cover a mandatory failure

	C
	Rejected: revise and resubmit; affected use held



Gate outcomes are letters A/B/C everywhere (meaning per Glossary V0.3 §1.5). The wording "gate decisions are words" is retired. Each outcome records scope, actual acceptor, authority, evidence and permitted use.
6 Gate families (O-DEC-109)
Three gate families exist. They are different decisions and are never merged; the table shows their typical alignment, and each project records its actual alignment in the BEP.
	Office stage gate (Manual V0.5 §2.1, eight gates)
	Basis-of-design gate (BBM-STD-12 C5)
	Authority gate (BBM-STD-57 §4)

	Strategic Need /​ Business Case (RIBA 0)
	G0 Basis
	none

	Brief /​ Information Requirements Approval (RIBA 1)
	G0 Basis
	none

	Concept Design Approval (RIBA 2)
	G1 Concept/​planning
	Concept /​ planning

	Coordination Freeze (RIBA 3)
	G2 Permit/​start activity (package preparation)
	Permit /​ final design (preparation)

	Issue for Review (RIBA 4)
	G2 Permit/​start activity (submission)
	Permit /​ final design

	Verified Construction Information Exchange (RIBA 5, procurement-dependent)
	G3 Construction
	Construction activity

	Handover Data Acceptance (RIBA 6)
	G4 Completion/​occupancy
	Completion /​ operation

	Operational Trigger /​ AIM Update Acceptance (RIBA 7)
	G5 Use/​renewal (e.g. Dubai Law 3/​2026 quality and safety certificate)
	none (owner renewal routes, BBM-STD-85)



Short form used in BBM-STD-12 C5: G1 = Concept/planning, G2 = Permit/final design, G3 = Construction activity, G4 = Completion/operation; G0 and G5 have no authority-gate equivalent.
Every gate outcome in all three families is a letter A/B/C (§5, O-DEC-107). Authority gates also record the authority's approval status (§7); an A/B/C outcome never replaces or proves an authority approval.
7 Approval status vocabulary (O-DEC-110)
The BBM-STD-57 §2/§4 set is canonical. BBM-STD-12 C4 statuses are detail values that map to it.
	Canonical status (BBM-STD-57)
	BBM-STD-12 C4 statuses mapped to it
	Rule

	Unverified
	Pending screening
	Applicability not yet established; silence is not exemption

	Planned
	Not started; In preparation
	No submission made

	Submitted
	Submitted; Under review
	Needs the actual receipt or application number

	Conditionally approved
	Approved with conditions
	Activity released only when the relevant conditions are checked closed

	Approved
	Approved
	Needs the authority's exact decision and scope

	Rejected
	Rejected; Revise/​resubmit
	Resubmission is a new submission record linked to the rejected one

	Expired
	Expired; Superseded
	Revalidation trigger recorded. Superseded = no longer valid because a later submission replaced it; keep the Superseded flag and link to the replacing record



One C4 value is not an approval status: Not applicable is an applicability decision in the BBM-STD-57 §2 Codes table (needs signed reason and authority).
8 Review tiers and issue severity
	Tier (O-DEC-108)
	Scope

	L1
	Discipline review inside the task team

	L2
	Cross-discipline review (coordination)

	L3
	Committee review (design/​quality committee)



The BIM Manager is a role, not a tier. Issue severity (BBM-STD-50 §7) is separate: S1 Critical, S2 Major, S3 Minor. S codes are severity, SU codes are suitability, A/B/C are gate outcomes, L1–L3 are review tiers; none is a RACI letter.
9 Acceptance
	Check
	Evidence

	One dictionary
	51, 66, Manual, 50, 68 carry a pointer to this document and no competing list

	Validation
	File-name, view-name, sheet and folder validators read their code lists from this dictionary's current revision

	Project mappings
	Every client-imposed code set has a one-to-one mapping in the BEP
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•  ISO 19650-1:2018 (information states and suitability concepts): https://committee.iso.org/standard/68078.html, checked 2026-11-04.
•  ISO 19650-2:2018 (delivery phase; formal delivery, authorisation and acceptance): https://committee.iso.org/standard/68080.html, checked 2026-11-04.
•  IMI Framework (formerly UK BIM Framework, renamed May 2025), resources including the Information Protocol template for BS EN ISO 19650-2 (Ed 6) and the UK National Annex code context: https://ukbimframework.org/resources/, checked 2026-11-04.
•  Office sources mapped: Manual V0.5 §2.1, §12.1, §12.3; Glossary V0.3 §1.5; BBM-STD-12 V0.2 C4, C5; BBM-STD-50 V0.3 §2, §7; BBM-STD-51 V0.2 §4; BBM-STD-57 V0.2 §2, §4; BBM-STD-66 V0.2 §1; BEP V0.5.
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