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Revision history
	Version
	Date
	Change

	V0.1
	2026-10-16
	First controlled draft

	V0.2
	2026-11-04
	Audit res-026 closure: §3 rebuilt as the ONE edition register (O-DEC-111) with international rows (G141), UAE instrument rows (G142), IMI Framework row (G140) and withdrawn BS 1192/​PAS 1192 family (G144); §4 code values moved to BBM-STD-93 (O-DEC-103/​104); §6 current drafts and BBM-STD-72/​75/​76 indexed (G143, G145); §5 licence register pointer to BBM-STD-94; references re-checked + cross-doc pointer pass + folder names without dots (O-DEC-149) + QMS patch res-033

	V0.3
	2026-11-05
	§3 rows settled from primary sources (O-DEC-153–O-DEC-161): ED-DM-9-1-1 thresholds, ED-DUBAI-BIM-STD version 1.4 /​ IFC4 /​ Appendix B, ED-DBC with the AR 225/​2024 parameters, ED-DXB-LAW-3-2026 gazette, ED-UAE-CRS Abu Dhabi EPSG codes, ED-ISO10002 date, ED-AUH-PLANNING and ED-UTILITY-REGS instruments; rule-based rows marked

	V0.4
	2026-11-05
	Standard watch no. 1 (RES-017) applied: ED-ISO19011 = ISO 19011:2026 edition 4, the 2018 edition withdrawn (O-DEC-184); new row ED-DM-11-9-1, DM circular 11-9-1 of 2026 applying ED-DXB-LAW-3-2026 (O-DEC-185); ED-SIRA settled on the SIRA Preventive Systems Manual (Administrative Resolution 13 of 2025) and the Security Plan Certificate service (O-DEC-186); ED-UAE-FLS records the reported ADCDA amendments circular, rule kept; ED-DUBAI-BIM-STD re-read on the DM package, still 1.4; wording: ED-COBIE (COBie V3.0 published 2023), ED-ISO12006-2 (confirmed 2020, to be revised), ED-UAE-CTL (corrigendum OG 821 checked, Art. 821/​823/​824 unchanged)



1 Purpose and control
Use one controlled office register to select current standards, resolve dependencies, validate container identities and establish permission to use software, content and licensed publications. The BIM Manager maintains the register; the document controller checks references; the office director approves adoption within office powers. Project departures need the actual appointment authority. Actual holders and deputies remain in the restricted Directory.
This document closes the drafting scope of SG-003, SG-015 and SG-095. It extends the existing glossary, Manual and BEP without changing issued baselines. The companion editable register contains blank input rows, a disk-derived current drafting inventory and a fictional SYN-P001 example. Inventory presence and a hash establish identity, not adoption. No office approval, entitlement or installed tool capability is asserted.
	Control
	Required entry

	Register identity
	RegisterID, revision, custodian, restricted CDE URI and effective date

	Adoption
	Prepared, independently checked and director decision IDs; exact approved files and hashes

	Review
	At material standard, appointment, tool, authority, licence or incident change and the glossary's 12-month office review cycle

	Change
	Stable ChangeID, prior/​new revision, impact, approval, notification and retest evidence



2 One master index and dependencies
Allocate each document or asset a stable ID before drafting. Record title, kind, revision, owner function, approval state, current master URI, issued-history URI, exact dependency IDs/revisions, next review date and evidence of approval. A companion form or native asset has a distinct AssetID linked to its parent standard. Markdown and DOCX are representations of the same controlled standard, not competing authorities. Record their source/build relationship and reconcile changes before issue.
All workbook file paths are relative to the office-rev root, one directory above xlsx; this base is stated on Read me. The workbook Master index is a baseline inventory of existing office standards, guides and their available companion assets at this drafting date. Standard IDs are BBM-STD-nn or BBM-STD-MIDP/TIDP, with the descriptive filename held separately. Companion AssetIDs have their own namespace and parent standard ID. A blank Next review date is an adoption hold, not a completed field. The Allocations table reserves 51, 55, 57, 52, 53, 54 and 56 for this queue. Planned entries have no current-release URI. Each new release is promoted into the index only after checking its actual pack, dependency revisions and decision. Do not label a proposed ID approved because the allocation exists.
	Dependency record
	Validation

	ConsumerID and revision
	Exists exactly once in the master index for the selected baseline

	RequiredID and revision
	Resolves to an available current source or a retained explicitly pinned issued baseline

	Applicability and reason
	Identifies affected clause, asset, project or exchange

	Impact and decision
	Changed dependency triggers owner assessment, same ChangeID and notified consumers



Library index snapshots (O-DEC-135). The shared family library index grows between reads, so every use quotes filename, row count, read date and full SHA-256. Recorded snapshots (read-only; owner of the index is the library-production owner, BBM-STD-69 §1 and BBM-STD-72 §2 cite these rows):
	Snapshot
	File
	Rows
	Read /​ modified
	SHA-256
	State

	LIB-IDX-S1
	Family CSV, filename not recorded; no longer on the share
	568
	read 2026-10-16
	ccb2ced96efd2e3b91cfaf70a5279dcd9800ca5a583ba3d6d94f9bbef9ceb38b
	History only

	LIB-IDX-S2
	02-LIBRARIES/​01-FAMILIES/​BBM-FAMILY-LIBRARY-INDEX.csv
	878
	read 2026-10-16
	6d4ecac1310377706ce3937e98a64a5fc097f0d07784a617d450691cd5ae45a4
	Superseded snapshot

	LIB-IDX-S3
	02-LIBRARIES/​01-FAMILIES/​BBM-FAMILY-LIBRARY-INDEX.csv
	889
	read 2026-11-04; modified 2026-10-29
	5b586168d9ff202f747b85bf14d0caaacbee48485bf24529aa5712d6cb504aaa
	Current at 2026-11-04



Library and share paths in this standard are written in the NN-NAME folder form without dots (O-DEC-149). A share that still carries an earlier dotted folder name maps one-to-one to the path written here; the file name, row count and SHA-256 identify the file.
Before a release, traverse every applicable dependency and current link, including companion forms and diagrams. Check exact case/path, revision, actual availability, approval and permitted audience. Zero unresolved IDs or broken current references are permitted within the released scope. An unbuilt future interface is an open condition, never an active approved dependency. Preserve historic issued files and their references. A baseline snapshot is retained with its manifest and decision evidence.
3 Adopted publications and precedence: the one edition register
Binding applicable law and authority conditions cannot be waived by a workbook or appointment. The commercial/legal owner records the actual appointment hierarchy; the technical team must not invent a universal order among contract documents. Within that agreed hierarchy, EIR fixes required exchanges, the BEP describes delivery and this office register controls the selected standards and aliases. Escalate conflicts and hold only the affected use.
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This section is the ONE edition and adoption register for the whole office standard set (O-DEC-111). Every other document cites a register ID below instead of restating an edition or date. BBM-STD-12 A3 (CODE-nnn) and BBM-STD-57 §2 (InstrumentID) reference these IDs. UAE requirement detail (thresholds, submission steps, evidence) lives in BBM-STD-85; this register holds only the edition facts. Where a value could not be confirmed from a primary source, the row states the dependence-free rule instead of an edition. All rows checked 2026-11-04. Project code applicability, editions/amendments, transition dates, jurisdiction and verified clauses are frozen in the project copy of this register before technical reliance; the newest publication is not automatically the adopted code (O-DEC-126).
International and professional publications
	ID
	Instrument
	Edition /​ status
	Date
	Office treatment
	Primary URL
	Checked

	ED-ISO19650-1
	ISO 19650-1 Concepts and principles
	2018, ed.1, in force. ISO/​DIS 19650-1 ed.2 at stage 40.93, not in force
	2018-12
	Concepts baseline; a draft never replaces the edition automatically
	https:/​/​www.iso.org/​standard/​68078.html
	2026-11-04

	ED-ISO19650-2
	ISO 19650-2 Delivery phase
	2018, ed.1, in force. ISO/​DIS 19650-2 at stage 40.93, not in force
	2018-12
	Delivery baseline (BEP, MIDP/​TIDP, formal delivery per 5.7, O-DEC-117)
	https:/​/​www.iso.org/​standard/​68080.html
	2026-11-04

	ED-ISO19650-3
	ISO 19650-3 Operational phase
	2020, ed.1
	2020-07
	Operational context (BBM-STD-52, 75)
	https:/​/​www.iso.org/​standard/​75109.html
	2026-11-04

	ED-ISO19650-4
	ISO 19650-4 Information exchange
	2022, ed.1
	2022-08
	Exchange review and acceptance (BBM-STD-50, 54, 64)
	https:/​/​www.iso.org/​standard/​78246.html
	2026-11-04

	ED-ISO19650-5
	ISO 19650-5 Security-minded approach
	2020, ed.1, confirmed 2025
	2020-06
	Security triage and plan in BBM-STD-87
	https:/​/​www.iso.org/​standard/​74206.html
	2026-11-04

	ED-ISO19650-6
	ISO 19650-6 Health and safety information
	2025, ed.1 (replaces PAS 1192-6)
	2025-01-13
	H&S information in BBM-STD-88
	https:/​/​www.iso.org/​standard/​82705.html
	2026-11-04

	ED-ISO7817-1
	ISO 7817-1 Level of information need
	2024, ed.1 (replaces EN 17412-1:2020)
	2024-06-20
	LOIN baseline (Glossary 1.3, BEP 6.5, BBM-STD-54, 89)
	https:/​/​www.iso.org/​standard/​82914.html
	2026-11-04

	ED-EN17412-1
	BS EN 17412-1:2020
	Withdrawn; replaced by ISO 7817-1:2024
	2020
	Keep only a contracted reference, with a successor mapping to ED-ISO7817-1
	https:/​/​standardsdevelopment.bsigroup.com/​projects/​2018-02659
	2026-11-04

	ED-ISO16739-1
	ISO 16739-1 IFC
	2024, ed.2 = IFC 4.3.2.0
	2024-03-22
	Office default exchange schema stays IFC 4.0.2.1 (IFC4 ADD2 TC1) Reference View; IFC 4.3.2.0 by recorded approval after a passing test exchange; IFC2x3 only when an appointment or authority profile requires it (O-DEC-105)
	https:/​/​www.iso.org/​standard/​84123.html
	2026-11-04

	ED-IDS
	buildingSMART Information Delivery Specification
	IDS 1.0 final
	June 2024
	Machine-readable alphanumeric LOIN checks (BBM-STD-54 §4.1, BBM-STD-89)
	https:/​/​github.com/​buildingSMART/​IDS/​releases
	2026-11-04

	ED-BCF
	buildingSMART BIM Collaboration Format
	BCF 3.0 final (bcfXML and BCF-API); BCF 2.1 (2017) fallback
	2021-06-18
	bcfXML 3.0 default; API after endpoint qualification; 2.1 via recorded field map (BBM-STD-50)
	https:/​/​github.com/​buildingSMART/​BCF-XML/​releases/​tag/​v3.0
	2026-11-04

	ED-IFC-VALIDATION
	buildingSMART IFC Validation Service
	Live service
	live
	Schema/​specification conformance before IDS and clash runs
	https:/​/​technical.buildingsmart.org/​services/​validation-service/​
	2026-11-04

	ED-ISO12006-2
	ISO 12006-2 Classification framework
	2015, ed.2, last reviewed and confirmed 2020; stage 90.92 to be revised, ISO/​DIS 12006-2.2 under development
	2015
	Classification framework behind Uniclass (BBM-STD-72)
	https:/​/​www.iso.org/​standard/​61753.html
	2026-11-05

	ED-ISO12006-3
	ISO 12006-3 Object-oriented information
	2022, ed.2
	2022-07-15
	Data dictionary framework (bSDD)
	https:/​/​www.iso.org/​standard/​74932.html
	2026-11-04

	ED-ISO23386
	ISO 23386 Property definition
	2020, ed.1, confirmed 2025
	2020-03
	Property definition attributes (BBM-STD-52, 54, 72)
	https:/​/​www.iso.org/​standard/​75401.html
	2026-11-04

	ED-ISO23387
	ISO 23387 Data templates
	2025, ed.2
	2025-09-22
	Data templates (BBM-STD-52, 54, 72)
	https:/​/​www.iso.org/​standard/​85391.html
	2026-11-04

	ED-ISO21597
	ISO 21597-1 and -2 Information container for linked document delivery
	2020 (both); -2 confirmed
	2020-11
	Linked-container exchange where an appointment requires it
	https:/​/​www.iso.org/​standard/​74389.html ; https:/​/​www.iso.org/​standard/​74390.html
	2026-11-04

	ED-ISO29481
	ISO 29481 Information delivery manual
	-1:2025 ed.3; -2:2025 ed.2; -3:2022
	2025 /​ 2022-09
	IDM method for exchange definitions (BBM-STD-74)
	https:/​/​www.iso.org/​standard/​88515.html ; https:/​/​www.iso.org/​standard/​81261.html
	2026-11-04

	ED-UNICLASS
	Uniclass 2015 (NBS)
	July 2026 release: Pr v1.43, Ss v1.43, SL v1.36, Ac v1.27
	2026-07
	Classification_Code + ClassificationTable/​Title/​Release (O-DEC-116); cite the release used
	https:/​/​uniclass.thenbs.com/​download
	2026-11-04

	ED-RIBA-POW
	RIBA Plan of Work
	2020 (current)
	2020
	Stage names
	https:/​/​www.riba.org/​work/​insights-and-resources/​riba-plan-of-work/​
	2026-11-04

	ED-ISO13567
	ISO 13567-1 and -2 CAD layers
	2017, ed.2 (both), confirmed
	2017-09
	CAD layer structure (BBM-STD-66)
	https:/​/​www.iso.org/​standard/​70181.html ; https:/​/​www.iso.org/​standard/​70182.html
	2026-11-04

	ED-ISO128-1
	ISO 128-1 TPD general principles of representation
	2020, ed.2
	2020-05
	Drawing principles (BBM-STD-67)
	https:/​/​www.iso.org/​search.html?q=ISO%20128-1
	2026-11-04

	ED-ISO7200
	ISO 7200 Title blocks and document headers
	2004, ed.2, confirmed 2025
	2004-02
	Title-block fields (BBM-STD-67)
	https:/​/​www.iso.org/​standard/​35446.html
	2026-11-04

	ED-ISO5457
	ISO 5457 Sizes and layout of drawing sheets
	1999 + Amd 1:2010; confirmed 2021
	1999 /​ 2010-06
	Sheet margins and layout (BBM-STD-67)
	https:/​/​www.iso.org/​standard/​29017.html ; https:/​/​www.iso.org/​standard/​46218.html
	2026-11-04

	ED-ISO216
	ISO 216 Paper sizes A and B series
	2007; confirmed 2021
	2007
	Sheet sizes (BBM-STD-67)
	https:/​/​www.iso.org/​standard/​36631.html
	2026-11-04

	ED-ISO10005
	ISO 10005 Quality plans
	2018, ed.3; confirmed 2023
	2018-06
	Quality plan structure (BBM-STD-68; office QMS BBM-STD-96, 97 QP-02)
	https:/​/​www.iso.org/​standard/​70398.html
	2026-11-04

	ED-ISO19011
	ISO 19011 Auditing management systems
	ISO 19011:2026, edition 4, published May 2026 (stage 60.60); ISO 19011:2018 withdrawn 27 May 2026 (O-DEC-184)
	2026-05
	Auditor competence and independence, audit programme guidance (BBM-STD-68; BBM-STD-96 §9.2 and §11; BBM-STD-97 QP-13)
	https:/​/​www.iso.org/​standard/​19011
	2026-11-05

	ED-ISO10006
	ISO 10006 Quality management in projects
	2017; confirmed 2023
	2017
	Project quality plans (BBM-STD-96 §8, BBM-STD-97 QP-02)
	https:/​/​www.iso.org/​standard/​70376.html
	2026-11-04

	ED-ISO10002
	ISO 10002 Complaints handling
	2018, ed. 3 (published 2018-07-16; confirmed 2023-12-11, stage 90.93)
	2018-07
	Complaints (BBM-STD-97 QP-12)
	https:/​/​www.iso.org/​standard/​71580.html
	2026-11-04

	ED-ISO10004
	ISO 10004 Customer satisfaction: monitoring and measuring (ed.2, confirmed 2023, stage 90.93)
	2018
	2018-07
	Client feedback and satisfaction KPIs (BBM-STD-97, BBM-STD-98)
	https:/​/​www.iso.org/​standard/​71582.html
	2026-11-04

	ED-LEED
	USGBC LEED
	Version per project registration
	per project
	Client-targeted rating only (BBM-STD-97 QP-06)
	https:/​/​www.usgbc.org/​leed
	2026-11-04

	ED-ISO9001
	ISO 9001 Quality management systems
	2026, ed.6 (replaces 9001:2015 + Amd 1:2024)
	2026-09-16
	Office QMS (BBM-STD-96, 97, 98) and QMS interface (BBM-STD-68); certificates to 2015 follow the certification body's transition period
	https:/​/​www.iso.org/​standard/​88464.html
	2026-11-04

	ED-ISO27001
	ISO/​IEC 27001 Information security management
	2022, ed.3 + Amd 1:2024
	2022-10 /​ 2024
	CDE/​service-provider security evidence (BBM-STD-56, 87)
	https:/​/​www.iso.org/​standard/​82875.html
	2026-11-04

	ED-ISO42001
	ISO/​IEC 42001 AI management system
	2023, ed.1
	2023-12
	AI governance (BBM-STD-92)
	https:/​/​www.iso.org/​standard/​42001
	2026-11-04

	ED-ISO55001
	ISO 55001 Asset management systems
	2024, ed.2 (2014 withdrawn)
	2024-07
	Asset-management interface (BBM-STD-02, 75)
	https:/​/​www.iso.org/​standard/​83054.html
	2026-11-04

	ED-ISO22057
	ISO 22057 EPD data templates for BIM; RICS WLCA
	ISO 22057:2022 (under revision); RICS whole life carbon assessment 2nd ed. effective 1 Jul 2024
	2022 /​ 2024-07-01
	Carbon data (BBM-STD-81)
	https:/​/​www.iso.org/​standard/​72463.html
	2026-11-04

	ED-PAS1958
	PAS 1958 Built environment data and information standards landscape. Guide
	PAS 1958:2026, current
	2026-03-31
	Data/​AI readiness reference (BBM-STD-92)
	https:/​/​knowledge.bsigroup.com/​search?query=PAS%201958
	2026-11-04

	ED-COBIE
	COBie (NIBS NBIMS-US)
	COBie 2.4 (NBIMS-US V3, 2015) default; COBie V3.0 published 2023 as part of NBIMS-US V4 (NIBS version history)
	—
	Delivered when the EIR requires; version as the EIR specifies; default COBie 2.4 unless the EIR names v3 (O-DEC-114)
	https:/​/​nibs.org/​nbims/​v4/​resources/​ ; https:/​/​nibs.org/​nbims/​v3/​cobie/​2-7
	2026-11-05

	ED-IMI
	IMI Framework (formerly UK BIM Framework, renamed May 2025) guidance
	Guidance Parts A–F archived (A/​D/​E ed.2 Feb 2021 retained as archived explanatory editions)
	2025-05
	Explanatory only; not UAE statute
	https:/​/​ukbimframework.org/​resources/​
	2026-11-04

	ED-INFO-PROTOCOL
	IMI Framework Information Protocol template for BS EN ISO 19650-2
	Template Ed 6 for new appointments; protocol guidance ed.3 (Aug 2022)
	2022 /​ live
	Protocol baseline for BBM-STD-56; the one dated entry all docs cite
	https:/​/​ukbimframework.org/​resources/​
	2026-11-04

	ED-CIC-PROTOCOL
	CIC BIM Protocol
	2nd ed. 2018, legacy (PAS 1192 era)
	2018
	Do not use for new appointments
	https:/​/​www.cic.org.uk/​shop/​cic-bim-protocol-2nd-edition
	2026-11-04

	ED-BS1192
	BS 1192 /​ PAS 1192 family; BS 8536
	WITHDRAWN: BS 1192:2007+A2:2016 16 Jan 2019; PAS 1192-2 18 Jan 2019; PAS 1192-3 18 Aug 2020; PAS 1192-5 1 Jul 2020; BS 1192-4 16 Sep 2022; PAS 1192-6 23 Jan 2025. BS 8536:2022 supersedes BS 8536-1/​-2
	as listed
	Successors ISO 19650-1/​-2/​-3/​-5/​-6. Legacy mapping only through §3.1; never cited as current
	https:/​/​knowledge.bsigroup.com/​products/​specification-for-information-management-for-the-capital-delivery-phase-of-construction-projects-using-building-information-modelling
	2026-11-04

	ED-REVIT
	Autodesk Revit supported releases and IFC exporter
	Supported 2024, 2025, 2026, 2027; 2023 out of Autodesk support (legacy, existing projects only with risk acceptance and upgrade plan); latest update 2027.3; IFC exporter 27.4.0.30 exports IFC4x3
	2026-09-15 /​ 2026-10-30
	Matrix in BBM-STD-91 (O-DEC-120); IFC 4.3 RV only after a test export from the project build passes the project IDS
	https:/​/​www.autodesk.com/​support/​account/​manage/​versions/​previous-versions ; https:/​/​github.com/​Autodesk/​revit-ifc/​releases
	2026-11-04



UAE instruments (requirement detail in BBM-STD-85; jurisdiction applicability per project through BBM-STD-57 and the BoD). There is no UAE federal BIM mandate, and no universal Abu Dhabi building-permit BIM threshold was found.
	ID
	Instrument
	Edition /​ status
	Date
	Office treatment
	Primary URL
	Checked

	ED-DM-196-207
	DM BIM circulars 196 (2013) and 207 (2015)
	Earlier circulars, cited by circular 9-1-2
	2013 /​ 2015
	Historical context only
	https:/​/​dmpmedia.dm.gov.ae/​uploads/​2023/​10/​تعميم-BIM-9-1-2.pdf
	2026-11-04

	ED-DM-CIRC-INDEX
	DM Building and Planning Circulars index
	Live official index (no dates per entry); the single DM circular index URL used by BBM-STD-57, 61 and 67
	live
	Watch source for new DM circulars (BBM-STD-57 §6)
	https:/​/​www.dm.gov.ae/​building-planning-circulars-2/​
	2026-11-04

	ED-DM-9-1-1
	DM circular 9-1-1 of 2021 on applying BIM
	Dated 23 Aug 2021. BIM for architectural and mechanical works: over 20 floors; over 200,000 sq ft; specialised buildings (hospitals, universities and the like); all government projects; all projects by a foreign office subsidiary. BIM for structural works: over 40 floors; over 300,000 sq ft; specialised buildings; buildings by a foreign office subsidiary (O-DEC-153)
	2021-08-23
	2021 BIM-use scope; permit submission scope is 9-1-2 /​ 9-1-3; follow the widest scope that applies
	https:/​/​dmpmedia.dm.gov.ae/​uploads/​2024/​11/​9-1-1-Application-of-Buildings-Information-Modelling.pdf
	2026-11-05

	ED-DM-9-1-2
	DM circular 9-1-2 BIM with new building permits
	Open BIM submission per the Dubai BIM Standard from 1 Jan 2024: over 20 floors (ARC) /​ 40 floors (STR); over 20,000 m² (ARC) /​ 30,000 m² (STR); specialised buildings (hospitals, universities); government projects except utility projects
	2023-10-13
	Permit BIM route in BBM-STD-57 §3 /​ BBM-STD-85
	https:/​/​dmpmedia.dm.gov.ae/​uploads/​2023/​10/​تعميم-BIM-9-1-2.pdf
	2026-11-04

	ED-DM-9-1-3
	DM circular 9-1-3 BIM with building permits
	From 1 Apr 2026: ARC + STR BIM with the permit for new buildings above G+12 or 15,000 m² or more; listed alterations (add/​remove floors, +1,500 m² or more, full redesign, change of main use, relocation on plot) with the application; other alterations: final BIM before the completion certificate; drawings extracted from the model
	2026-01-15; effective 2026-04-01
	Permit BIM route in BBM-STD-57 §3 /​ BBM-STD-85
	https:/​/​www.dm.gov.ae/​wp-content/​uploads/​2026/​02/​Circular-9-1-3.pdf
	2026-11-04

	ED-DUBAI-BIM-STD
	Dubai BIM Standard and Model Attribute Matrix
	Version 1.4 (changelog 8 Jun 2026): IFC4 schema, .ifc files (§6.1.1); authority Revit setup "Dubai BIM E-Submission (IFC4)Reference View"; Appendix B Model Attribute Matrix issued with 1.4 (file 5 Jun 2026, no separate version number; BIMStandardVersion = 1.4.0); Appendix A Model Element Matrix; Appendix C Usage Codes; DM IDS DMBIM_IDS_V1; CRS EPSG:3997 with DMD elevations; ZIP within the platform maximum (150 MB per changelog) (O-DEC-154); package re-read 2026-11-05 (server date 2 Nov 2026): still Version 1.4.0
	2026-06-08
	Office preset EXP-DM-PERMIT-IFC4-<rev> (O-DEC-131) built on the authority setup; re-checked at project start and before each submission (BBM-STD-85 §9)
	https:/​/​buildindubai.gov.ae/​bim ; https:/​/​api.buildindubai.gov.ae/​assets/​BIM/​Documents/​DubaiBIMStandards.zip
	2026-11-05

	ED-DBC
	Dubai Building Code (Decree 45/​2021) as amended by DM Administrative Resolution No. 225 of 2024
	Apply the DBC plus all DM amending resolutions in force at permit submission. AR 225/​2024 (issued 16 Jul 2024, published 13 Aug 2024, in force 30 days later) applies to plots of 250 m² or less only and permits seven parameter changes: no lifts for G+2 or lower with 100 occupants or fewer; ground-floor lift lobby 1.8 m; typical-floor corridor and lift lobby 1.5 m; one shared WC per shop of 100 m² or less; no bulky-waste area; no recycling area in the refuse room; no extra 300 mm bay width beside columns/​walls (O-DEC-155)
	2021 /​ 2024-08-13
	Design basis (BBM-STD-12, 57, 85); DBC clause per AR 225 item recorded at project start
	https:/​/​www.dm.gov.ae/​municipality-business/​laws-and-orders/​ ; https:/​/​dmpmedia.dm.gov.ae/​uploads/​2024/​08/​قرار-إداري-رقم-225-لسنة-2004.pdf
	2026-11-05

	ED-DXB-LAW-3-2026
	Dubai Law No. 3 of 2026 on the Quality and Safety of Buildings (emirate law)
	Issued 27 Feb 2026; Official Gazette issue 764, 12 Mar 2026; in force 60 days after publication, i.e. from 11 May 2026 (O-DEC-156); Quality & Safety Certificate after 20 years from completion, valid 10 years (5 years if 40+ years); applied by DM circular 11-9-1 of 2026 (ED-DM-11-9-1)
	2026-02-27
	Asset-life obligation for existing buildings (BBM-STD-75, 76, 85); not a design-permit rule
	https:/​/​dlp.dubai.gov.ae/​Legislation%20Reference/​2026/​Law%20No.%20%283%29%20of%202026%20Concerning%20the%20Quality%20and%20Safety%20of%20Buildings.html
	2026-11-04

	ED-DM-11-9-1
	DM circular (11-9-1) of 2026 applying Law No. 3 of 2026 (parent row ED-DXB-LAW-3-2026), with the guidance manual "Building Quality and Safety Certificate" (attachment 11-9-1-1, May 2026)
	Dated 1 Oct 2026, applies from that date: owners of buildings completed 20 or more years ago obtain a Building Quality and Safety Certificate after a technical assessment against the DM technical checklist and remediation of any defects found; valid 10 years (under 40 years since completion) or 5 years (40 years or more), renewed in the last 90 days before expiry by the same procedure; phased, first multi-storey buildings over 40 years old, each owner on DM notice with a deadline; the owner appoints an engineering office licensed in Dubai whose classification matches the building height; applications on the Build in Dubai e-service; Civil Defence and SIRA compliance certificates mandatory
	2026-10-01
	Existing-building assessment service: BBM-STD-75 §7, BBM-STD-85 §4 and §11; the office acts only as the appointed engineering office (O-DEC-185)
	https:/​/​dmpmedia.dm.gov.ae/​uploads/​2026/​10/​11-9-1.pdf ; https:/​/​dmpmedia.dm.gov.ae/​uploads/​2026/​10/​11-9-1-1.pdf
	2026-11-05

	ED-UAE-FLS
	UAE Fire & Life Safety Code of Practice
	September 2018 edition; emirate amendments (rule-based, O-DEC-160): the edition plus the emirate Civil Defence amendments current at project start, checked on the emirate Civil Defence code page and circulars, recorded in BEP §1.12. Abu Dhabi: ADCDA Circular No. 3 of 2026 (12 Mar 2026, 54 decisions amending the 2018 edition) and an ADCDA smoke-management duct circular are reported by secondary sources only; neither was found on adcda.gov.ae on 2026-11-05, so they apply only from the ADCDA text obtained at project start
	2018-09
	Fire basis; Fire_Rating per O-DEC-119
	https:/​/​www.dcd.gov.ae/​portal/​preventive-safety/​uae-fire-and-life-safety-code-of-practice.jsp ; https:/​/​www.adcda.gov.ae/​
	2026-11-05

	ED-ADIBC
	Abu Dhabi International Building Codes
	The ADIBC edition published by DMT and in force at project start (2013 edition at 2026-11-05; Executive Council Resolution 7C 26/​2013, effective 1 Oct 2013); a later edition is rule-based (O-DEC-160): checked on the DMT codes page at project start
	2013
	Abu Dhabi design basis
	https:/​/​www.dmt.gov.ae/​-/​media/​Project/​DMT/​DMT/​Codes/​3-ADIMC-2013_1-12-2013.pdf
	2026-11-04

	ED-ADC9-2026
	Abu Dhabi UPPC Circular No. 9 of 2026, supervision consultant and contractor roles
	Issued 2026-10-14
	2026-10-14
	Supervision roles, phase notices and joint phase reports (BBM-STD-97 QP-09)
	https:/​/​www.Project.ae/​en/​article/​c2qm3pn-uppc-issues-circular-streamline-construction
	2026-11-04

	ED-DDA-CIRC-400
	DDA Circular 400: Drawings Submission Standards
	Dated 29 Sep 2021: A1 DWF drawings, monochrome except perspectives and shaded area diagrams, discipline tabs and sheet naming; the current Final Design Approval service checklist governs where it differs
	2021-09-29
	DDA drawing submissions (BBM-STD-57 §3, BBM-STD-61, BBM-STD-67)
	https:/​/​dda.gov.ae/​-/​media/​436DDFA50D8B4AC1A075607917327616.pdf
	2026-11-04

	ED-AUH-PLANNING
	Abu Dhabi planning and area-definition regulations
	Abu Dhabi Capital Development Code (DMT) for plots in Abu Dhabi City Municipality; Al Ain and Project: the DMT development code of that municipality, title and edition recorded at project start (O-DEC-161)
	2022
	Area definitions (BBM-STD-58 §3.1)
	https:/​/​www.dmt.gov.ae/​-/​media/​Project/​DMT/​DMT/​E-Library/​Abu-Dhabi-Capital-Development-Code.pdf
	2026-11-05

	ED-UTILITY-REGS
	Utility authority regulations (Dubai DEWA; Abu Dhabi utility)
	Dubai: DEWA Regulations for Electrical Installations, 2017 Edition. Abu Dhabi: Abu Dhabi Emirate Guideline for Infrastructure Services Standards, 2nd edition, January 2017 (index of ADDC /​ RSB water and electricity codes). Other utilities (district cooling, gas, telecom): the provider's current regulation recorded at project start (O-DEC-161)
	2017 /​ 2017-01
	MEP design basis, utility separations and NOCs (BBM-STD-50 §4.1, BBM-STD-57 §3, BBM-STD-60 §3)
	https:/​/​www.dewa.gov.ae/​-/​media/​DEWA_Regulations_for_Electrical_Installations_2017_Edition.ashx ; https:/​/​www.dmt.gov.ae/​-/​media/​Project/​DMT/​ADM/​E-Library/​Abu-Dhabi-Emirate-Guideline-for-Infrastructure-Services-Standards.pdf
	2026-11-05

	ED-ADM-BIM
	ADM BIM Code of Practice; Infrastructure Documentation Guidelines; Infrastructure BIM Object Catalogue
	CoP Oct 2020 (cover v1, headers v1.1); Guidelines v1.0 Oct 2020; Object Catalogue v2.0 May 2021
	2020–2021
	Abu Dhabi BIM context; infrastructure scope
	https:/​/​www.dmt.gov.ae/​adm/​-/​media/​Project/​DMT/​ADM/​E-Library/​0001-Jan-2022-Doc/​ADM-BIM-005Code-of-Practice.pdf
	2026-11-04

	ED-ESTIDAMA
	Estidama Pearl Rating System
	Private projects minimum 1 Pearl; government-funded minimum 2 Pearl
	2025-01-08
	Statutory minimum (BBM-STD-57, 81, 85)
	https:/​/​www.dmt.gov.ae/​en/​adm/​Media-Centre/​News/​08Jan2025
	2026-11-04

	ED-ALSAFAT
	Al Sa'fat Dubai Green Building System
	2nd edition: Silver Sa'fa mandatory for all new buildings in Dubai
	2023-01
	Statutory minimum (BBM-STD-57, 81, 85)
	https:/​/​www.dm.gov.ae/​municipality-business/​al-safat-dubai-green-building-system/​
	2026-11-04

	ED-UAE-PDPL
	Federal Decree-Law No. 45 of 2021 on the Protection of Personal Data
	Active; executive regulations as listed on uaelegislation.gov.ae at project start
	effective 2022-01-02
	Personal data (BBM-STD-03, 90)
	https:/​/​uaelegislation.gov.ae/​en/​legislations/​1972
	2026-11-04

	ED-UAE-CTL
	Federal Decree-Law No. 25 of 2025 (Civil Transactions Law)
	Decennial liability Art. 821 (engineer and contractor jointly, 10 years from delivery); Art. 823 bars exemption clauses; Art. 824 three-year claim period. Contracts signed before 1 Jun 2026: Federal Law 5/​1985 Art. 880. Corrigendum in the annex of Official Gazette No. 821 (14 Apr 2026) checked: the text as corrected lists no change to Art. 821–824, and the official Art. 821, 823 and 824 read as quoted here (read 2026-11-05)
	effective 2026-06-01
	Retention minimum 10 years after handover + 3 years; final schedule ruled by the legal owner (BBM-STD-90)
	https:/​/​uaelegislation.gov.ae/​en/​legislations/​4011 ; https:/​/​www.lexismiddleeast.com/​gazette/​UnitedArabEmirates/​2026_821_Annex/​en
	2026-11-05

	ED-SIRA
	Dubai SIRA security-system requirements
	Law No. 12 of 2016 regulating the security industry in Dubai and its Implementing Bylaw (Resolution No. 1 of 2018); SIRA Administrative Resolution No. 13 of 2025 approving the Preventive Systems Manual (issued 14 Apr 2025, in force on Official Gazette publication): camera views, ANPR, access control, guards and system health monitoring per establishment type; Security Plan Certificate (SPC) and Security System Certification e-services (O-DEC-186)
	2025-04-14
	Security-system drawings follow the Manual chapter for the establishment type; the SPC is stamped by a SIRA-licensed security consultancy and installer, not by the office; classified per BBM-STD-87; SIRA compliance certificate needed for ED-DM-11-9-1
	https:/​/​dlp.dubai.gov.ae/​Legislation%20Reference/​2025/​Administrative%20Resolution%20No.%20%2813%29%20of%202025%20Approving%20the%20Preventive.html ; https:/​/​www.sira.gov.ae/​en/​services/​security-plans-certification
	2026-11-05

	ED-UAE-CRS
	Project coordinate reference systems (CRS register keys CRS-DXB, CRS-AUH, CRS-OTH in BBM-STD-86 §2)
	Dubai: DLTM, EPSG:3997 "WGS 84 /​ Dubai Local TM", required by the Dubai BIM Standard 1.4 §4.1.2; WGS 84 based, so no datum transformation for WGS 84 data; vertical DMD (Port Rashid datum, no EPSG code) (O-DEC-157). Abu Dhabi: WGS 84 (ITRF2000) /​ UTM 40N EPSG:32640 east of 54°E, UTM 39N EPSG:32639 west of 54°E; vertical Ras Ghumays, EPSG:5843 (O-DEC-159)
	2026-06-08 /​ 2023-02
	Register and procedure in BBM-STD-86; zone chosen from the plot, never one emirate-wide code
	https:/​/​epsg.io/​3997 ; https:/​/​admobility.gov.ae/​services/​-/​media/​As-Built-Data-Submission-Standards.pdf ; https:/​/​epsg.io/​5843
	2026-11-05

	ED-UAE-NATIONAL
	UAE federal BIM mandate
	None found; MoEI green building codes (2022) noted
	2022
	No federal BIM rule is assumed
	https:/​/​www.Project.ae/​en/​details/​1395303033593
	2026-11-04




For every adoption record retain publisher/source URL, standard identifier, edition, published/draft/withdrawn status, national adoption, jurisdiction, applicable clauses, contractual incorporation, verification date, licensed access route and approving function. Licensed texts remain in their controlled permitted store. No copied paid-standard paragraphs or licence keys belong here.
ISO clause pointers are paraphrased reading directions: ISO 19650-1 clause 5 concerns requirements; ISO 19650-2 clauses 5.1.4 and 5.1.5 concern the project's information standard and production methods. Check the licensed publication before a formal compliance assertion. Public catalogue pages prove scope and edition only.
3.1 Legacy transition worksheet
The following is an office mapping method for BS 1192-era project records, not a reproduced BS code table. Compare the actual historical project standard and signed appointment before adopting a mapping. Preserve every issued literal and its original meaning.
	Legacy component or record
	Current treatment
	Approval or unsupported condition

	Project; originator
	PROJ; ORG
	Verify allocated project/​organisation codes; CLIENT is an additional office token, not a claimed BS requirement

	Volume or system; level or location
	VOLUME; LEVEL
	Confirm scope and granularity; no inferred ZZ for an unknown division

	Type; role; number
	TYPE; ROLE; NUMBER
	Validate code meanings and number namespace; use a controlled alias where meanings differ

	Legacy suitability/​status literal
	Preserve old literal and meaning; map to one SU value only after use/​recipient review
	A similar-looking S code is not an automatic ISO/​SU equivalent. Unknown meaning holds the affected use

	Legacy revision literal
	Retain issued literal; use an explicit old-to-new revision map for future issues
	Rnn continues where already adopted; other series need the appointment authority's decision, never an arithmetic conversion

	Internal ORG-PROJ-DISC-PHASE-SEQUENCE
	Mapped internal WIP alias only, linked to one eight-token external identity; never issued (O-DEC-102)
	Trade maps to role through BBM-STD-93; the PHASE token is retired (stage is permitted-use metadata); multi-token descriptors require registered handling



The workbook Legacy map records the old literal, current meaning, applicability, ChangeID, approver, effective revision and retained-history URI. For the synthetic example, LEG-SYN-COORD is explicitly defined as coordination in its fictitious project standard and maps to SU-COORD. It is not represented as a BS 1192 code. Review and notify all affected CAD, Revit and CDE users before the next applicable exchange.
4 Shared naming and metadata register
Retain O3-POL-01 in Clash Matrix section 2 and BEP 8.3 as the existing policy authority (O-DEC-102). This table implements that decision, rather than establishing another grammar. Register one appointment mapping when the recipient requires different tokens or codes. The eight-token external identity is CLIENT-ORG-PROJ-VOLUME-LEVEL-TYPE-ROLE-NUMBER.ext. Tokens are uppercase, separated by single hyphens; NUMBER has four digits; the approved extension is lowercase. Revision and suitability are metadata.
Code values live in one place: BBM-STD-93 Code dictionary (O-DEC-103, O-DEC-104). This section keeps only the token order and validation rules. Short summary for orientation; BBM-STD-93 governs where they differ:
	Token /​ metadata
	Rule (values in BBM-STD-93)

	CLIENT /​ ORG /​ PROJ
	Allocated project lists; fictional example CLI /​ OFF /​ P001, never a client identity

	VOLUME /​ LEVEL
	Registered zone and level codes; ZZ only where whole scope is explicitly adopted; never omit a token

	TYPE
	Registered container type codes (e.g. M3 model, DR drawing)

	ROLE
	One-letter ROLE from BBM-STD-93 (A, S, M, E, L, P, F, I, C, G, Q, W, Z). A trade alias is not a role code

	NUMBER
	Four digits, unique in the recorded numbering namespace

	Extension
	Lowercase; same-stem variants map to one logical container and declared source revision

	Revision
	R00 initial WIP, then R01, R02…, expanding beyond R99; per container, never recycled; unchanged containers keep their revision (O-DEC-113)

	Suitability
	SU-WIP, SU-COORD, SU-INFO, SU-REVIEW, SU-ISSUE only; mapping to UK National Annex S0–S7/​A/​B/​CR in BBM-STD-93 (O-DEC-104)

	CDE state
	WIP, Shared, Published, Archive. Distinct from workspace WIP/​PRODUCTION/​DEPLOYED folders

	Release evidence
	Exact identity/​revision, source/​export manifest, permitted use, author/​checker/​authoriser, recipients and separate receiving decision



These SU codes are local. They are not ISO/national-annex suitability codes, issue severities or RACI letters. SU-ISSUE does not prove statutory approval or recipient acceptance. An .ifc extension does not mean issued for construction.
CAD, Revit and CDE use the same external register. Retain internal view names DISC-LEVEL[-ZONE]-TYPE-DESC (3-letter discipline code from BBM-STD-93), sheet numbers DISC-CAT-INDEX (1-letter ROLE prefix from BBM-STD-93) and the registered STD00-STARTING-VIEW exception under Manual 12.3/BEP 8.3. Preserve approved legacy WIP aliases through a one-to-one alias-to-external-ID map. Never rename issued records to clean up a convention.
4.1 Validation fixtures
The workbook Test pack specifies positive and adverse cases for a future CAD/Revit/CDE validation implementation. Expected outcomes below are test specifications, not executed host evidence.
	Case
	Input
	Expected result and reason

	N01
	CLI-OFF-P001-Z01-L01-M3-A-0001.ifc
	Accept syntax and dictionary membership when manifest/​revision/​permission checks also pass

	N02
	CLI-OFF-P001-Z01-M3-A-0001.ifc
	Reject missing LEVEL; no token shift

	N03
	CLI-OFF-P001-Z01-L01-M3-A-001.ifc
	Reject sequence width

	N04
	CLI-OFF-P001-Z01-L01-M3-A-0001-R01.ifc
	Reject revision embedded in external identity

	N05
	CLI-OFF-P001-Z99-L01-M3-A-0001.ifc
	Reject unregistered volume even when a regex matches

	N06
	Same container and revision, conflicting payload hashes
	Reject unrecorded overwrite; investigate source/​history

	N07
	Same stem .rvt and .ifc, same manifest source
	Permit declared representations; still test schema and receiver

	N08
	Revision R02 followed by R01 as new issue
	Reject regression unless expressly retrieving retained historical evidence

	N09
	SU-COORD requested for fabrication
	Hold incompatible intended use; naming alone cannot authorise it

	D01
	Consumer points to an absent dependency ID
	Reject release until allocation/​source is resolved

	D02
	Consumer pins old issue, master now newer
	Preserve issued pin; assess migration rather than silently upgrade



A validator checks lexical syntax, code dictionaries, identity/representation uniqueness, metadata, revision history, dependency resolution and intended-use authority separately. Regex alone is insufficient. A future implementation must run every case in all affected tools and record exact versions and actual outputs before claiming enforcement.
5 Rights and licensed access
The licence and credential register itself is owned by BBM-STD-94; this section states the office rule only. The rights steward records EntitlementID, holder function/account reference, product/content/publication, provider and licence instrument/version, covered installations/users, authorised uses/recipients, expiry/renewal/review dates, evidence URI and restrictions. Store credentials only in the approved credential store. The register contains a non-secret reference, never a password, key, token or activation code.
Software permission, ability to open a file, third-party content redistribution rights and access to a paid standard are different checks. Record each separately. A valid software seat does not authorise redistribution of a family library, a standards PDF or model IP. Apply ISO 19650-5:2020 security context proportionately. Actual licence particulars follow the signed instrument, not this template.
	Fictional record
	Permission decision

	ENT-SYN-01, modelling software
	Internal named-user use only; renewal and installation evidence pending. No actual vendor entitlement asserted

	ENT-SYN-02, external content
	Internal evaluation only; no client or public redistribution until rights owner clears the exact item

	ENT-SYN-03, standards access
	Licensed-reader access at controlled portal; citation allowed within terms; do not redistribute the full publication



On expiry, revoked access, changed recipients or changed terms, the steward alerts the owner and holds the affected new use. Retention and retrieval of existing records follow the actual instrument and records/legal owner, not assumed immediate deletion.
6 Reference reconciliation and controlled migration
The current guide headers cite Manual V0.1 and BEP V0.2 while the current controlled drafts are Manual V0.5 and BEP V0.5; Manual V0.2/V0.3 and BEP V0.3/V0.4 are historical baselines. Do not bulk-rewrite other lanes' guides or issued project packs. The Migration table records each actually observed stale guide reference, its source line, proposed current target, exact dependency revision, affected steps, responsible guide owner, compatibility review, approval and effective revision. The row state remains Pending owner revision; the old reference is resolved as a historical baseline and the proposed target is a current draft, not an approved migration. Current draft paths must resolve; historical citations remain visibly historical until that owner's controlled revision is adopted.
A second conflict is retained Manual 12.3 wording that appears to prescribe the legacy five-token external filename. BEP 8.3, O3-POL-01 and O-DEC-102 settle this: legacy internal alias only, never issued; external eight-token identity; PHASE token retired. Record W1-C01 in the office decisions log and carry this interpretation in the project naming annex. Do not silently edit the source Manual.
Migration sequence: identify affected references; compare meanings; verify target availability/rights; obtain the controlling decision; revise the owner's draft and linked plans using one ChangeID; independently retest; notify recipients and retain the prior issue. If the newer document is still a draft, do not imply office adoption. BBM-STD-72/75/76 V0.1 are draft dependencies: index them in the Master index with draft state (BBM-STD-72, BBM-STD-75, BBM-STD-76 at their current draft revision); consumers pin the draft revision until adoption.
7 Acceptance and activation
	Check
	Evidence required

	Index and dependency integrity
	Every current ID unique, all required pinned revisions accessible, zero unresolved current references and a dated manifest

	Naming and representations
	Test pack actual outputs, code-register revision, alias map, revision/​suitability/​state and manifest checks

	Rights
	In-date evidence for actual use, account/​seat allocation and every intended recipient; no credentials in the register

	Migration
	Impact, authority, effective revision, notification and independent retest; issued originals preserved

	Adoption
	Director/​appointment decisions and actual authorised custodians. Draft review is not project mobilisation



The present pack supplies the method, editable forms and filled examples. Native CAD/Revit/CDE validation, real entitlements, office adoption and project receiving tests are NOT EXECUTED. Activate only the actual affected uses after their records and evidence are complete.
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